1. MASTER CONTROL UNIT

모델 : TOA, TS-D1000-MU

(1) 기  능

본 기기는 유선 디지털 회의 시스템 용 마스터 제어 장치로 LAN 케이블을 이용하여 간단히 의장용 유닛과 의원용 유닛을 최대 32개까지 연결 할 수 있어야한다. 추가 확장을 위해 최대 5개의 SUB 제어장치를 추가할 수 있고 따라서 최대 246개까지 의장/의원용 장치를 연결 할 수 있어야한다. 또한 FBS(Feedback Suppression)을 탑재하여 음향 피드백을 효과적으로 제어 할 수 있으며 다음과 같은 규격에 준한다.

(2) 성  능

- Power Source : 100 - 240 V AC, 50/60 Hz (use of the supplied AC adapter)

- Power Consumption : 60 W or less

- Audio Transmission System :	Time division multiplexing (TDM), 10 channels 16-bit PCM, 32 kHz sampling frequency

- MIC Input : -54 dB (*2), 600 Ω, unbalance, φ6.3 mm phone jack (2P)

- Output LINE : -10 dB (*2), 10 kΩ, unbalance, φ6.3 mm phone jack (2P)

REC : -10 dB (*2), 10 kΩ, unbalance, RCA pin jack, monaural

HEADPHONES : φ3.5 mm mini jack, monaural

- Number of Connectable Chairman/Delegate Units : 32 units

- Number of Connectable Sub Control Units : 5 units

- Maximum Cable Distance : 50 m (between Master control unit and terminal                                       Chairman/Delegate unit at end of daisy chain) (*3)

1 m (3.28 ft) (between Master control unit and                                    Sub control units) (Use the cable supplied with the                                  Sub control unit.)

- Maximum Number of Open Microphones : 2 chairman units, 8 delegate units

- Chairman/Delegate Units Terminal : RJ45 connector ×2

- Sub Control Units Terminal : RJ45 connector

- Recording Ports : USB-A

- Recording Function : Recordings can be made to a USB memory device (*4) or                            the internal memory.

- Recording format : MP3 (MPEG-1 Audio Layer-3), monaural

- Sampling frequency : 32 kHz, Bit rate: 128 kbps

- Network I/F : 10BASE-T/100BASE-TX (Automatic-Negotiation)

- Network Protocol : TCP, HTTP, DHCP, ARP (APIPA), UDP (mDNS)

- Network Connector : RJ45 connector

- Weight : 2.2 kg

- 동등 또는 이상 품이어야 한다.